Structure Maintenance Checklist

Structure No.:	District:
Inspected By:	Date of Inspection:
Structure Location:	County:

Item No.	Item	Maint. Needed	Item No.	Item	Maint. Needed
1.	Repair damaged guardrail.	9.	Fill in erosion on sideslopes and banks.
2.	Repair/replace signs.	10.	Fill in erosion at culvert ends.
3.	Clean debris from expansion device.	11.	Remove silt from barrels.
4.	Sweep the deck/open plugged floor drains.	12.	Remove excess silt between culvert wings.
5.	Remove debris from girder, caps, and bearings.	13.	Patch bridge deck.
6.	Remove debris from channel.	14.	Seal cracks.
7.	Cut and remove trees from channel.	15.	Pressure wash deck, rails, joints, and drains.
8.	Fill in washout under approach slab.	16.	Other:

Remarks:

NDOT Form 27, July 17